|  |  |
| --- | --- |
| **JBOD** |  |
|  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Product Name** | **Configuration** | **Drive Type** | **Interface** | **Drive Capacity (TB)** | **# of Drives** | **Total Capacity (TB)** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Ultrastar Data60 | Chassis Dual | HC DC310 | SAS | 6  | 60 | 360  |
| Ultrastar Data60 | Chassis Dual | HC DC320 | SAS | 8  | 60 | 480  |
| Ultrastar Data60 | Chassis Dual | He10-8 | SAS | 8  | 60 | 480  |
| Ultrastar Data60 | Chassis Dual | He10 | SAS | 10  | 60 | 600  |
| Ultrastar Data60 | Chassis Dual | He12 | SAS | 12  | 60 | 720  |
| Ultrastar Data60 | Chassis Dual | He14 | SAS | 14  | 60 | 840  |
| Ultrastar Data60 | Chassis Single | HC DC320 | SATA | 8  | 60 | 480  |
| Ultrastar Data60 | Chassis Single | He10 | SATA | 10  | 60 | 600  |
| Ultrastar Data60 | Chassis Single | He12 | SATA | 12  | 60 | 720  |
| Ultrastar Data60 | Chassis Single | He14 | SATA | 14  | 60 | 840  |
|   |   |   |   |   |   |   |
| Ultrastar Data60 | Chassis Dual | HC DC310 | SAS | 6  | 24 | 144  |
| Ultrastar Data60 | Chassis Dual | HC DC320 | SAS | 8  | 24 | 192  |
| Ultrastar Data60 | Chassis Dual | He10-8 | SAS | 8  | 24 | 192  |
| Ultrastar Data60 | Chassis Dual | He10 | SAS | 10  | 24 | 240  |
| Ultrastar Data60 | Chassis Dual | He12 | SAS | 12  | 24 | 288  |
| Ultrastar Data60 | Chassis Dual | He14 | SAS | 14  | 24 | 316  |
|   |   |   |   |   |   |   |
| **Product Name** | **Type** | **Drive Type** | **Interface** | **Drive Capacity (TB)** | **# of Drives** | **Total Capacity (TB)** |
| Ultrastar Data102 | Chassis Dual | HC DC310 | SAS | 6  | 102 | 612  |
| Ultrastar Data102 | Chassis Dual | HC DC320 | SAS | 8  | 102 | 816  |
| Ultrastar Data102 | Chassis Dual | He10-8 | SAS | 8  | 102 | 816  |
| Ultrastar Data102 | Chassis Dual | He10 | SAS | 10  | 102 | 1020  |
| Ultrastar Data102 | Chassis Dual | He12 | SAS | 12  | 102 | 1224  |
| Ultrastar Data102 | Chassis Dual | He14 | SAS | 14  | 102 | 1428  |
| Ultrastar Data102 | Chassis Single | He10 | SATA | 10  | 102 | 1020  |
| Ultrastar Data102 | Chassis Single | He12 | SATA | 12  | 102 | 1224  |
| Ultrastar Data102 | Chassis Single | He14 | SATA | 14  | 102 | 1428  |
|   |   |   |   |   |   |   |
| Ultrastar Data102 | Chassis Dual | HC DC310 | SAS | 6  | 60 | 360  |
| Ultrastar Data102 | Chassis Dual | HC DC320 | SAS | 8  | 60 | 480  |
| Ultrastar Data102 | Chassis Dual | He10-8 | SAS | 8  | 60 | 480  |
| Ultrastar Data102 | Chassis Dual | He10 | SAS | 10  | 60 | 600  |
| Ultrastar Data102 | Chassis Dual | He12 | SAS | 12  | 60 | 720  |
| Ultrastar Data102 | Chassis Dual | He14 | SAS | 14  | 60 | 840  |
| Ultrastar Data102 | Chassis Single | He10 | SATA | 10  | 60 | 600  |
| Ultrastar Data102 | Chassis Single | He12 | SATA | 12  | 60 | 720  |
| Ultrastar Data102 | Chassis Single | He14 | SATA | 14  | 60 | 840  |