|  |  |
| --- | --- |
| **JBOD** |  |
|  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Product Name** | **Configuration** | **Drive Type** | **Interface** | **Drive Capacity (TB)** | **# of Drives** | **Total Capacity (TB)** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Ultrastar Data60 | Chassis Dual | HC DC310 | SAS | 6 | 60 | 360 |
| Ultrastar Data60 | Chassis Dual | HC DC320 | SAS | 8 | 60 | 480 |
| Ultrastar Data60 | Chassis Dual | He10-8 | SAS | 8 | 60 | 480 |
| Ultrastar Data60 | Chassis Dual | He10 | SAS | 10 | 60 | 600 |
| Ultrastar Data60 | Chassis Dual | He12 | SAS | 12 | 60 | 720 |
| Ultrastar Data60 | Chassis Dual | He14 | SAS | 14 | 60 | 840 |
| Ultrastar Data60 | Chassis Single | HC DC320 | SATA | 8 | 60 | 480 |
| Ultrastar Data60 | Chassis Single | He10 | SATA | 10 | 60 | 600 |
| Ultrastar Data60 | Chassis Single | He12 | SATA | 12 | 60 | 720 |
| Ultrastar Data60 | Chassis Single | He14 | SATA | 14 | 60 | 840 |
|  |  |  |  |  |  |  |
| Ultrastar Data60 | Chassis Dual | HC DC310 | SAS | 6 | 24 | 144 |
| Ultrastar Data60 | Chassis Dual | HC DC320 | SAS | 8 | 24 | 192 |
| Ultrastar Data60 | Chassis Dual | He10-8 | SAS | 8 | 24 | 192 |
| Ultrastar Data60 | Chassis Dual | He10 | SAS | 10 | 24 | 240 |
| Ultrastar Data60 | Chassis Dual | He12 | SAS | 12 | 24 | 288 |
| Ultrastar Data60 | Chassis Dual | He14 | SAS | 14 | 24 | 316 |
|  |  |  |  |  |  |  |
| **Product Name** | **Type** | **Drive Type** | **Interface** | **Drive Capacity (TB)** | **# of Drives** | **Total Capacity (TB)** |
| Ultrastar Data102 | Chassis Dual | HC DC310 | SAS | 6 | 102 | 612 |
| Ultrastar Data102 | Chassis Dual | HC DC320 | SAS | 8 | 102 | 816 |
| Ultrastar Data102 | Chassis Dual | He10-8 | SAS | 8 | 102 | 816 |
| Ultrastar Data102 | Chassis Dual | He10 | SAS | 10 | 102 | 1020 |
| Ultrastar Data102 | Chassis Dual | He12 | SAS | 12 | 102 | 1224 |
| Ultrastar Data102 | Chassis Dual | He14 | SAS | 14 | 102 | 1428 |
| Ultrastar Data102 | Chassis Single | He10 | SATA | 10 | 102 | 1020 |
| Ultrastar Data102 | Chassis Single | He12 | SATA | 12 | 102 | 1224 |
| Ultrastar Data102 | Chassis Single | He14 | SATA | 14 | 102 | 1428 |
|  |  |  |  |  |  |  |
| Ultrastar Data102 | Chassis Dual | HC DC310 | SAS | 6 | 60 | 360 |
| Ultrastar Data102 | Chassis Dual | HC DC320 | SAS | 8 | 60 | 480 |
| Ultrastar Data102 | Chassis Dual | He10-8 | SAS | 8 | 60 | 480 |
| Ultrastar Data102 | Chassis Dual | He10 | SAS | 10 | 60 | 600 |
| Ultrastar Data102 | Chassis Dual | He12 | SAS | 12 | 60 | 720 |
| Ultrastar Data102 | Chassis Dual | He14 | SAS | 14 | 60 | 840 |
| Ultrastar Data102 | Chassis Single | He10 | SATA | 10 | 60 | 600 |
| Ultrastar Data102 | Chassis Single | He12 | SATA | 12 | 60 | 720 |
| Ultrastar Data102 | Chassis Single | He14 | SATA | 14 | 60 | 840 |